Using the Linux I2C Tools

i2cdetect -l

i2cdetect -y -r 2

i2cdump -y 2 0x68